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[bookmark: _Toc191978931]Introduction
[bookmark: _Hlk116463103]The Ontario Ministry of Natural Resources and Forests contracted Airborne Imaging to acquire and deliver digital elevation data derived from airborne LiDAR (Light Detection and Ranging) to cover various regions in Ontario.
This report covers the Timmins area, collected during the spring of 2024. The report focuses on LiDAR acquisition details, such as flight parameters, project control, ground truthing results, data processing technique and deliverables.
The contracted area for the Timmins area is 3,191.7 km².
[image: Map of the contracted Timmins area.]
[bookmark: _Toc191978932]Project Schedule & Personnel
The ground control occurred during the spring of 2024. The surveyor collecting ground truth points during this period was Alistair Lornie. The Lidar data was collected in three missions. See table below for a list of missions.
A typical Lidar acquisition crew consisted of one Lidar Operator and one Pilot.
[bookmark: _Toc191978933]LiDAR System & Flight Parameters
One Riegl VQ-1560ii was used to collect the Lidar data. The system was installed in Revolution Flight’s Cessna Caravan call sign N331RF.
Below is a table of the lifts with their flight parameters.
[image: Table with lifts, dates and flight parameters.]
Table 1: Project Parameters for the Timmins area.
	Riegl VQ1560-ii
	Flight plan

	Altitude
	 1650m AGL

	Field of View (FOV)
	 60°

	Air Speed
	 150 Kts

	Pulse Rate
	 2200 kHz

	Sidelap
	 20%

	Point Density
	 > 8 pts/m2



The flight lines were designed optimally to maximize time online versus time in turn.


Below is a map of the flight lines including cross-ties.
[image: Map of the flight lines over the Timmins project area.]


Below is a map of the flight line footprints.
[image: Map of the flight line footprints.]
Riegl VQ1560-ii (Blue), spring 2024
[bookmark: _Toc191978934][bookmark: _Hlk174517572]Project Control / Datum
Several baselines were measured by GPS static occupation between Can-Net Continuously Operating Reference Stations (CORS), existing NRCan 3D Passive Control Monuments, and Ontario COSINE control points, as well as newly established points by Airborne Imaging. The existing control used for the Timmins area consisted of one Can-Net station and two NRCan passive stations.
Appendix A contains a list of Control Points and their published coordinates.
Appendix B shows the coordinate list of deliverable check points.
Appendix C shows the published station coordinate sheets.
The datum used for processing the Ground Control and all subsequent Lidar data are the Nad83 CSRS (epoch 2010.0) horizontal datum and the CGVD2013 vertical datum (CGG2013 undulation model).


Below is an overview map of the control stations.
[image: Overview map of the Timmins control stations.]Figure 1 Control Points for MNRF Timmins

[bookmark: _Toc191978935]Check Points
RTK GPS
In order to meet the recommended ASPRS minimum number of points for a 3191.7 square kilometer project, RTK points were surveyed in areas distributed throughout the project. A minimum of 59 NVA and 48 VVA points were required to meet ASPRS standards. Real Time Kinematic points are individual points surveyed on open terrain. Our surveyor collected GPS data mounted on a pole while receiving real time differential corrections from the GPS receiver positioned over a nearby control point.
111 points were surveyed on the Timmins project. Of these, 57 points were over non-vegetated ground conditions for NVA accuracy reporting and 54 of them were over vegetated areas for VVA accuracy reporting. Pictures of these RTK points (as well as the existing control) are provided with this report in the folder labeled “Control_Point_Pictures”. These points are used just for the vertical accuracy assessment of the Lidar point cloud and were not used to determine any vertical shift applied to the point cloud. 
[image: Map of the NVA (yellow) and VVA (green) check points over the Timmins project area.]
Figure 2 NVA (Yellow) and VVA (Green) Check Points

[bookmark: _Toc191978936]Trajectory Processing
The aircraft trajectory positioning for the missions over the Timmins area were processed using the Precise Point Positioning (PPP) technique.
PPP is a positioning technique that removes and models GNSS system errors via precise satellite orbit data and clock corrections that are applied to the trajectory post mission, providing centimeter level positional accuracy without the use of ground base stations.
The TerraPOS software by Terratec was used to postprocess the PPP solutions to produce final kinematic trajectories accurate to 5 centimeters for each flight mission.
The horizontal datum used is Nad83 CSRS UTM zone 17 with the CGVD2013 vertical datum (CGG2013 undulation model).
[bookmark: _Toc191978937]LiDAR Data Processing
[bookmark: _Toc356382075][bookmark: _Toc50621095][bookmark: _Toc109974151][bookmark: _Toc191978938]Calibration Procedures
After each mission, the field project manager creates the preliminary calibrated point cloud with each sensor’s set boresight values for each mission. Proprietary QC tools using the Lastools software are run on each mission to check for coverage, relative accuracy, point density, etc… If any data is found to be not meeting specifications, or coverage missing, the field crew is immediately notified and the areas affected reflown as soon as possible.
This preliminary calibrated point cloud is inspected in conjunction with the kinematic ground truth points to apply bulk shifts if necessary and further refine the calibration by applying corrections to the preliminary calibrated strips. The refined calibration is done using Bayesmap’s StripAlign software. Intensity values are also normalized by mission to be 16 bits (0 to 65535).
[bookmark: _Toc50621096][bookmark: _Toc109974152][bookmark: _Toc191978939]Data Tiling and Classification
The raw LiDAR data is processed into calibrated point cloud strips corresponding to flight lines. For ease of data manipulation, the strips are combined and saved in tiles of 1 km by 1 km. The format the strips and tiles are saved in is .Laz version 1.4. The tiling scheme is based on the UTM17 projection at the even kilometers.
The tiled point cloud is then processed with a series of algorithms to separate the “most-likely” ground returns from other returns. The point classification is done using a product by the TerraSolid software running on MicroStation Connect called TerraScan and TerraModeler.
In addition to our regular field QC and calibration procedures, we also generate various raster products using the Lastools software to assess coverage and calibration accuracy.
[bookmark: _Toc50621098][bookmark: _Toc109974154][bookmark: _Toc191978940]Point Cloud Manipulation
The TerraScan software uses macros that are set-up to measure the angles and distances between points to determine what classification a point should be: ground, vegetation, noise, other.  The angle and distance values in the macros can be adjusted to be more or less aggressive with the classification of points by varying the incidence angles and estimated distances among neighboring points.  The lower points are generally classified as ground returns, with the points above classified as undefined (class 1). Outliers and noise described in the table below are normally clouds, outliers or atmospheric noise in the data that are separated into above or below the ground level (high point or low points).
After the automated macro is run to determine classes, a systematic visual inspection is performed to fine tune the ground definition.  To better understand areas for improvement for the ground surface, the points that are classified as ground are used to create viewable TINs and grid surfaces.  These surfaces are inspected for areas that appear rough, artificially flattened or truncated, no data areas, or have other viewable errors.
In cleaning up ground points, the focus is concentrated in areas where few ground points have been left in the bare earth model and the ground appears rough or lower and flatter than it may be in reality.  The scarcity of ground points may be a result from no penetration through a dense vegetation layer, water bodies, low reflectivity objects, or too aggressive values with the macro.  A manual/visual inspection of these areas plays a major role in resolving any issues or irregularities with the bare earth model. 
Once the first edits are completed, a one-meter grid of the ground surface is re-exported and hill shade images produced to QC the edited ground surface. This QC step is done iteratively as many times as necessary. Once the point cloud data has reached a satisfactory level of classification accuracy, the final deliverables are produced.
[bookmark: _Toc191978941]Water Classification & Hydro-Flattening
[bookmark: _Toc356382076][bookmark: _Toc50621097][bookmark: _Toc109974153]Once the ground class has reached the final level of classification accuracy, the water delineation process is initiated. The rivers and water bodies are digitized as break lines according to USGS specifications of a minimum of 8000 m² for water bodies and 30 m nominal width for streams and rivers. Ponds and lakes have their elevations set constant to just below ground. Stream and river hydro lines are collected using the downstream method. Once all hydro lines have been collected for an area, the ground points inside the hydro lines are classified to class 9 – Water. The ground points outside of the hydro lines but within 35 cm are classified to class 20 – Ignored ground (near breaklines). Using the TIN of class 2 (ground points), the hydro lines are used as constraints to generate the final 50 cm hydro-flattened DEMs in ESRI Ascii format, then converted to 32bit GeoTIFF format with the Global Mapper software.
[bookmark: _Toc191978942]Class definitions
The classification follows the ASPRS classification codes. The table below shows the classes for the delivered point cloud.


Table 2: ASPRS Point Classes
	Classification Value
	Description

	1
	Unclassified

	2
	Ground

	6
	Building

	7
	Low Points

	9
	Water

	17
	Bridge Decks

	18
	High Points

	20
	Ignored Ground (breakline proximity)

	21
	Snow

	22
	Temporal exclusion


[bookmark: _Toc191978943]Deliverables
See below for a table of the folder structure and description of each deliverable.
DIFF
50cm rasters of flight lines differences, 1 X 1 km tiles in 32bit GeoTIFF format
e.g. 1km174460534702024LTIMMINS_diff.tif
DTM
Hydro-flattened 50cm Bare Earth DEMs, 1 X 1 km tiles in 32bit GeoTIFF format
e.g. 1km174460534702024LTIMMINS.tif
METADATA
Metadata files for Breaklines, DEM, LAS and Project in .XML format
e.g. TIMMINS_2024_Lidar_metadata_LAS.xml
POINTCLOUD
Point cloud data, 1 X 1 km tiles in .LAZ format 1.4
e.g. 1km174460534702024LTIMMINS.laz
PROJECT_POLYGON
Shape files of: Lift_metadata, Hydro_breaklines, Project_extent & Tile_index
e.g. Mission_5124125a_z17.shp


[bookmark: _Toc191978944]Vertical Accuracy Assessment

Non-Vegetated Vertical Accuracy (NVA)
Below is a summary of the statistics between the point cloud TIN from the ground class and the NVA points surveyed on flat hard surfaces:
	Number of points:
	57
	

	Average dz:
	0.019
	m

	Minimum dz:
	-0.056
	m

	Maximum dz:
	+0.063
	m

	Average magnitude:
	0.032
	m

	Root mean square:
	0.037
	m

	Std deviation:
	0.032
	m

	
	
	

	NVA Vertical Accuracy (95%):
	0.073
	m



For a complete listing of the RTK points and their differences, please refer to the provided spreadsheet named "Timmins_NVA_Accuracy_z17_Final.xlsx".
As seen in the NVA comparison above, the accuracy observed of 0.082 m meets the project requirement of QL0 NVA vertical accuracy of 9.8 cm (95%). 

Vegetated Vertical Accuracy (VVA)
The elevations of the points surveyed in various vegetated land cover types were compared to the Lidar ground surface. Since the elevation differences for this type of accuracy does not follow a normal distribution, the percentile method is used and not the 95% confidence level. For the 54 VVA points surveyed, sorting the absolute differences from the smallest to the largest gives the accuracy at the 95th percentile (using the linear interpolation between closest ranks method). For this sample, the 51st and 52nd largest difference are respectively 10.7 and 11.2 cm. 
For this project, the VVA accuracy is therefore 10.88 cm.
This meets the required specifications of 15.0 cm (the QL0 VVA specification).
For a complete listing of the kinematic points and their differences, please refer to the provided spreadsheet named "Timmins_VVA_Accuracy_z17_Final.xlsx".
[bookmark: _Toc191978945]Conclusion
This is the final report covering the Timmins Lidar project. Topics such as field operations, control, data processing and final accuracy results were explained. Both the non-vegetated and vegetated vertical accuracies meet the QL0 requirement.
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[bookmark: _Toc191978946][bookmark: _Hlk174517756]Appendix A - Control Points – Published Coordinates
Timmins - Control Station Coordinates
	Station
	Easting
	Northing
	h
	H (CGVD2013)
	Status
	Comments

	653050
	472635.122
	5379248.454
	254.921
	292.075
	Published
	NRCan 3D Passive Monument

	963015
	460128.674
	5374569.535
	288.301
	325.294
	Published
	NRCan 3D Passive Monument

	TIM3  
	472065.564
	5369403.472
	252.419
	289.561
	Published
	Can-Net CORS Station

	1988-30
	475640.353
	5388764.274
	250.812
	287.949
	Temporary
	Airborne Intermediate Control

	1988-31
	452370.114
	5390209.687
	275.580
	312.552
	Temporary
	Airborne Intermediate Control

	1988-32
	467988.120
	5368087.125
	251.907
	289.009
	Temporary
	Airborne Intermediate Control

	1988-33
	457754.108
	5359066.825
	274.775
	311.681
	Temporary
	Airborne Intermediate Control

	1988-34
	476209.285
	5355563.614
	267.564
	304.606
	Temporary
	Airborne Intermediate Control

	1988-35
	485230.186
	5370786.922
	248.901
	286.102
	Temporary
	Airborne Intermediate Control

	1988-36
	495556.100
	5377597.781
	251.752
	289.043
	Temporary
	Airborne Intermediate Control

	1988-37
	504204.236
	5385075.455
	243.111
	280.410
	Temporary
	Airborne Intermediate Control



Nad83(CSRS), epoch 2010
UTM Zone 17


[bookmark: _Toc191978947]Appendix B – RTK Survey & Control Check
	Point
	Julian Day
	Northing
	Easting
	Height
	Description

	963015
	106
	5374569.535
	460128.674
	325.294
	Base

	2040
	106
	5375347.065
	472060.651
	278.617
	NVA

	2009
	106
	5359552.724
	458902.296
	309.980
	NVA

	2012
	106
	5364348.958
	466128.404
	290.763
	NVA

	2014
	106
	5366496.877
	462461.375
	307.970
	NVA

	2015
	106
	5366578.620
	449773.970
	327.992
	NVA

	2025
	106
	5368919.459
	464823.760
	282.605
	NVA

	2026
	106
	5371211.007
	462554.863
	288.796
	NVA

	2027
	106
	5375825.200
	460009.061
	364.078
	NVA

	2029
	106
	5379064.666
	454520.113
	287.616
	NVA

	2030
	106
	5381253.711
	453436.408
	289.495
	NVA

	2031
	106
	5368926.865
	470244.805
	287.554
	NVA

	2033
	106
	5371432.160
	470467.706
	277.224
	NVA

	2037
	106
	5371777.041
	474435.053
	282.568
	NVA

	2042
	106
	5375335.596
	467247.585
	285.461
	NVA

	2057
	106
	5367602.938
	475579.075
	301.956
	NVA

	2091
	106
	5386775.269
	453387.748
	296.773
	NVA

	2092
	106
	5383691.151
	447006.780
	302.970
	NVA

	2093
	106
	5389625.613
	448777.448
	317.010
	NVA

	2094
	106
	5393551.274
	451177.943
	283.969
	NVA

	2107
	106
	5361478.713
	461993.599
	302.377
	NVA

	2108
	106
	5366591.831
	455927.733
	322.003
	NVA

	2600
	106
	5390224.588
	452370.082
	311.125
	NVA

	3009
	106
	5359546.422
	458888.508
	309.044
	VVA

	3012
	106
	5364379.028
	466112.612
	290.451
	VVA

	3014
	106
	5366512.763
	462451.291
	306.885
	VVA

	3016
	106
	5366592.572
	449773.687
	327.488
	VVA

	3025
	106
	5368910.942
	464834.796
	282.699
	VVA

	3026
	106
	5371209.559
	462541.633
	288.747
	VVA

	3027
	106
	5375849.617
	460014.614
	365.864
	VVA

	3029
	106
	5379076.408
	454503.226
	286.724
	VVA

	3030
	106
	5381265.187
	453434.020
	289.613
	VVA

	3031
	106
	5368918.154
	470243.420
	287.484
	VVA

	3033
	106
	5371504.670
	470417.091
	274.381
	VVA

	3037
	106
	5371787.934
	474467.903
	283.965
	VVA

	3040
	106
	5375333.730
	472067.073
	277.981
	VVA

	3042
	106
	5375339.063
	467255.422
	284.973
	VVA

	3058
	106
	5367598.008
	475592.419
	302.143
	VVA

	3091
	106
	5386779.484
	453400.309
	296.102
	VVA

	3092
	106
	5383677.025
	447013.085
	302.711
	VVA

	3093
	106
	5389630.060
	448763.896
	317.512
	VVA

	3094
	106
	5393588.415
	451162.529
	284.607
	VVA

	3106
	106
	5371355.310
	467228.530
	287.982
	VVA

	3107
	106
	5361527.395
	461960.770
	302.926
	VVA

	3108
	106
	5366583.774
	455929.633
	321.431
	VVA

	3600
	106
	5390234.820
	452370.171
	310.424
	VVA

	1988-34
	107
	5355563.614
	476209.285
	304.606
	Base

	2059
	107
	5363657.409
	475214.728
	298.535
	NVA

	2060
	107
	5360007.445
	476496.076
	309.128
	NVA

	2095
	107
	5353497.202
	475565.278
	303.209
	NVA

	2097
	107
	5349598.213
	476719.167
	315.542
	NVA

	2098
	107
	5355382.631
	479007.693
	306.676
	NVA

	2099
	107
	5352287.148
	479811.331
	312.252
	NVA

	3060
	107
	5360018.599
	476506.180
	309.435
	VVA

	3061
	107
	5363643.492
	475226.638
	298.802
	VVA

	3095
	107
	5353508.534
	475539.349
	302.979
	VVA

	3098
	107
	5355356.956
	479014.763
	306.303
	VVA

	3099
	107
	5352296.207
	479809.832
	310.778
	VVA

	1988-33
	107
	5359066.825
	457754.108
	311.681
	BASE

	2001
	107
	5353131.143
	446845.451
	337.185
	NVA

	2003
	107
	5353511.719
	449159.822
	332.600
	NVA

	2004
	107
	5356136.223
	451763.873
	327.743
	NVA

	2006
	107
	5349803.871
	457350.109
	318.652
	NVA

	2008
	107
	5355414.322
	458321.140
	317.087
	NVA

	2016
	107
	5357943.408
	467878.986
	297.742
	NVA

	2017
	107
	5354823.559
	464976.965
	306.333
	NVA

	3001
	107
	5353107.190
	446864.355
	335.745
	VVA

	3003
	107
	5353527.928
	449146.565
	332.464
	VVA

	3004
	107
	5356133.476
	451754.508
	327.508
	VVA

	3005
	107
	5357203.108
	454489.504
	333.740
	VVA

	3006
	107
	5349816.726
	457351.618
	317.519
	VVA

	3016
	107
	5357949.714
	467880.305
	297.514
	VVA

	3017
	107
	5354829.102
	465003.134
	306.913
	VVA

	3096
	107
	5354471.796
	470703.623
	319.828
	VVA

	653050
	108
	5379248.454
	472635.122
	292.075
	BASE

	2045
	108
	5378652.104
	472638.437
	284.238
	NVA

	2049
	108
	5374439.772
	478046.280
	297.853
	VVA

	2050
	108
	5377951.759
	479740.725
	296.721
	NVA

	2052
	108
	5387289.596
	476341.824
	293.068
	NVA

	2053
	108
	5388794.069
	475655.317
	288.723
	NVA

	2056
	108
	5395029.424
	474522.716
	288.472
	NVA

	2061
	108
	5383487.285
	478253.751
	285.807
	NVA

	2062
	108
	5365932.146
	480589.937
	309.777
	NVA

	2063
	108
	5369539.192
	478959.170
	320.751
	NVA

	2068
	108
	5366095.695
	486374.128
	335.115
	NVA

	2101
	108
	5361734.955
	490887.137
	283.096
	NVA

	3045
	108
	5378665.352
	472627.637
	283.515
	VVA

	3049
	108
	5374419.331
	478046.429
	298.026
	VVA

	3050
	108
	5377928.172
	479736.877
	297.408
	VVA

	3052
	108
	5387291.490
	476373.016
	292.852
	NVA

	3053
	108
	5388764.292
	475640.345
	287.977
	VVA

	3056
	108
	5395044.386
	474527.487
	288.971
	VVA

	3061
	108
	5383475.034
	478267.948
	285.194
	VVA

	3062
	108
	5365935.715
	480583.050
	309.184
	VVA

	3063
	108
	5369544.687
	478973.597
	319.963
	VVA

	3068
	108
	5366078.720
	486385.858
	334.472
	VVA

	3101
	108
	5361725.119
	490876.199
	282.863
	VVA

	1988-36
	108
	5377597.781
	495556.100
	289.043
	BASE

	2069
	108
	5371066.619
	485507.272
	290.040
	NVA

	2072
	108
	5376574.849
	487292.619
	288.976
	NVA

	2077
	108
	5377640.452
	495204.837
	292.358
	NVA

	2078
	108
	5380842.323
	499126.937
	294.877
	NVA

	2079
	108
	5383170.048
	502599.254
	289.899
	NVA

	2083
	108
	5375945.300
	504165.174
	284.214
	NVA

	2084
	108
	5372832.951
	502504.333
	284.594
	NVA

	2086
	108
	5375439.593
	511218.355
	277.398
	NVA

	2088
	108
	5379917.477
	507984.252
	295.213
	NVA

	2100
	108
	5385738.455
	499345.668
	289.693
	NVA

	2103
	108
	5392658.767
	498399.520
	337.034
	NVA

	3078
	108
	5380855.466
	499141.346
	294.298
	VVA

	3079
	108
	5383175.875
	502608.085
	289.072
	VVA

	3080
	108
	5371164.921
	489759.044
	290.819
	VVA

	3083
	108
	5375920.449
	504155.980
	283.388
	VVA

	3084
	108
	5372837.670
	502511.177
	284.618
	VVA

	3088
	108
	5379911.775
	507971.361
	295.335
	VVA

	3090
	108
	5385588.844
	508001.337
	289.376
	NVA

	3104
	108
	5373607.672
	493768.747
	287.227
	VVA


[bookmark: _Toc191978948]Appendix C – Published Station Coordinate Sheets
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Flight Date h[‘l:y" Lift H:“'s AGL.m s("k:: P":;Zm s“(:;’“ (::;) '::‘::r Operator |Aircraft Co| Aircraft |Sensor|
2024-05-04] 125 |5124125a] 75 1650 | 150 | 2200 332 | 60 | AFox | A Gruber |Revolution| N331RF |Rieglbl]
2023-05-07| 128 |5124128a| 6.4 1650 | 150 | 2200 332 | 60 | AFox | A Gruber |Revolution| N331RF [Riegl51]
2023.05.09] 130 |5124130a] 9.1 1650 | 150 | 2200 332 | 60 | A Fox | A Gruber |Revolution| N331RF | Riegl51]
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D
-37.155 + 0.009 292.079 2001-01-01 M01707

Vertical Data

Use the value of H from the coordinates above.




image9.png
Government  Gou
of Canada  du Canada

nt

Natural Resources Canada

Station Marker

Marker Type Inspected in | Established by Status Comments
Brass/bronze 1995 Canadian Good None
tablet or cap geodetic survey

- nrcan

Location

Accessible by passenger car or light truck and a walk of less than 50 m.

Timmins located at timmins airport on m.o.t. Property,approx 100 m sse from the new
terminal building. Mkd by br tab set in top of conc mon, 45.7 cm in dia and protruding 5
cm above grd Ivl. Mkr is stpd "653050". A subsurface mkr was set. The tablet is about 1 m
e of the e ditch of northbound rd, 41.4 m ne of a "parking keep left" sign for north bound
traffic. 26.8 m se of power pole, .6 m at a magnetic bearing 0f 285 degrees from an
orange cylindrical witness sign. The ref a and b are along a fence on w side, 46 cm away.
In 1992, 653050b was not located. Suitable for gps.

Location

TIMMINS LOCATED AT TIMMINS AIRPORT ON M.O.T. PROPERTY,APPROX 100 M SSE FROM
THE NEW TERMINAL BUILDING. MKD BY BR TAB SET IN TOP OF CONC MON, 45.7 CM IN DIA
AND PROTRUDING 5 CM ABOVE GRD LVL. MKR IS STPD "653050". A SUBSURFACE MKR
WAS SET. THE TABLET IS ABOUT 1 M E OF THE E DITCH OF NORTHBOUND RD, 41.4 M NE
OF A "PARKING KEEP LEFT" SIGN FOR NORTH BOUND TRAFFIC. 26.8 M SE OF POWER
POLE, .6 M AT A MAGNETIC BEARING OF 285 DEGREES FROM AN ORANGE CYLINDRICAL
WITNESS SIGN. THE REF A AND B ARE ALONG A FENCE ON W SIDE, 46 CM AWAY. IN 1992,
6530508 WAS NOT LOCATED. SUITABLE FOR GPS.
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Station Report - 963015

Station 1 of 1
Site Identification
Name Province NTS map Unique Provincial Network
sheet. Number Identifier
TIMS Ontario 042A12 963015 CBN
TIMMINS

Station Coordinates

Coordinates Reference | Vertical Datum Geoid Epoch
Frame.
geo NADB3(CSRS) CGVD2013 CGG2013a 2010
Latitude Longitude h (metres)
N48° 31' 22.600286" + WB81° 32 23.932895" = 288.300 + 0.0059m
0.0019m 0.0014m
Ve (mm/y) VA (mmly) Vh (mm/y)
-2.08 +0.26 1.98 +0.18 6.14 + 0.80
N (metres) H (metres) Published aaltDe and project
-36.993 = 0.008 325.203 2023-09-05 M18-020

Vertical Data

Vertical  [Elevation (m) |  Order Gravity Published | Project ID
Datum (mGal)
CGVD2013 | 325.203 1st 980822.67 2013 H13ML1311
(2010.0)
CGVD28 325.259 1st 980932.61 1999 NOU99
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Marker Type | Inspectedin | Established by Status Comments
Self centering 2015 Canadian Good None
plate geodetic survey
- nrcan

Accessible by passenger car or light truck and a walk of less than 50 m.

imins concrete pillar with steel top plate on top of large rock outcrop on southwest side
of municipal road (formerly highway no. 576), 10.8 km northwest of junction with highway
no. 101, 2.1 km northwest of steel culvert for "twentythree mile® creek, 0.5 km southeast
of kreiner road (road to kamiskotia ski resort), 94 m northwest of power line crossing
highway, opposite point on highway 81.8 m southeast of "kamiskotia ski resort road” sign
for northbound traffic, 31.2 m from centre line of highway, 7.6 m southeast of centre of
approach to northeast, about 4.5 m above highway level.

TIMMINS CONCRETE PILLAR WITH STEEL TOP PLATE ON TOP OF LARGE ROCK OUTCROP
ON SOUTHWEST SIDE OF MUNICIPAL ROAD (FORMERLY HIGHWAY NO. 576), 10.8 KM
NORTHWEST OF JUNCTION WITH HIGHWAY NO. 101, 2.1 KM NORTHWEST OF STEEL
CULVERT FOR "TWENTYTHREE MILE" CREEK, 0.5 KM SOUTHEAST OF KREINER ROAD
(ROAD TO KAMISKOTIA SKI RESORT), 94 M NORTHWEST OF POWER LINE CROSSING
HIGHWAY, OPPOSITE POINT ON HIGHWAY 81.8 M SOUTHEAST OF "KAMISKOTIA SKI
RESORT ROAD" SIGN FOR NORTHBOUND TRAFFIC, 31.2 M FROM CENTRE LINE OF
HIGHWAY, 7.6 M SOUTHEAST OF CENTRE OF APPROACH TO NORTHEAST, ABOUT 4.5 M
ABOVE HIGHWAY LEVEL.
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Station Report - CTM3

Station 1 of 1

Site Identification

Name Province NTS map Unique Provincial Network
sheet Number Identifier
CANNET- Ontario 042A06 cm3 CANNET
TIM3

Station Coordinates

Coordinates Reference | Vertical Datum Geoid Epoch
Frame
geo NADB3(CSRS) | CGVD2013 CGG2013a 2010
Latitude Longitude h (metres)
N4g° 28' 37.701535" + W81° 22" 40.719657" + 252.416 = 0.0009m
0.0006m 0.0003m
Vo (mmjy) VA (mmly) Vh (mm/y)
-2.08 = 0.00 1.95 + 0.00 5.78 = 0.00
N (metres) H (metres) FUEER=I et dpiect
-37.144 = 0.009 289.560 2021-05-07 M21-003

Vertical Data

Use the value of H from the coordinates above.

Station Marker

Marker Type

Inspected in | Established by

Status

Comments

Unknown

Cannet

None
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