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[bookmark: _Toc398015543][bookmark: _Toc393099763][bookmark: _Toc424024572]Purpose 

This document provides additional information to support the use of geospatial data.  The Physical Model Diagram provides a visual representation of the relationships in the data class. The Data Change History lists all the modelling and access changes that have occurred during the lifecycle of the data class. A data description identifying table and field names is available upon request.
[bookmark: _Toc424024573]Need Assistance?

Please contact LIO Support at lio@ontario.ca or 705-755-1878 if you require help.
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Data Class Change History

[bookmark: DCN]Data Class Name: Tower
[bookmark: DCShortN]Data Class Short Name: TOWER
	Date 
YYYY-MM-DD
	Details of Change

	2008
	Data class description changed - received new description from BDI.

	2006
	New GUT: Meteorological Tower

	1996
	NEW Data Class for NRVIS 1.0 to capture former Ontario Base Map (OBM) features.
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Data Description

Please refer to the metadata record for the data description. 
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Physical Model Diagram for:
Tower (TOWER)
Model Effective Date 2012-JUN-14
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TOWER_FT

OGF_ID: NUMBER(13) NOT NULL

CLASS_SUBTYPE: VARCHAR2(75) NOT NULL
CLASS_SUBTYPE_NUM: NUMBER(7) NOT NULL
TOWER_IDENT: VARCHAR2(11) NULL

OFFICIAL_NAME: VARCHAR2(75) NULL
PURPOSE_OF_TOWER_DESCR: VARCHAR2(7S) NULL.
RADIO_CALL_SIGN: VARCHAR2(10) NULL
HEIGHT_ABOVE_GROUND_NUM: NUMBER(102)NULL.
GROUND_ELEV_ASL_NUM:NUMBER(10) NULL
TOWER_FACE_SIZE_NUM: NUMBER(8.2) NULL
MANUFACTURER_NAME: VARCHAR2(35) NULL

MODEL NUMBER:VARCHAR2(15) NULL
TOWER_CONSTRUCTION_DATE: DATE NULL.
LAST_TOWER_INSPECT_DATE: DATE NULL
POWER_AVAILABLE_IND: VARCHAR2(3) NULL
ARPORT_RESTRICTION_IND: VARCHAR2(3) NULL
UPGRADING_REQUIRED_IND:VARCHAR2(3) NULL
TOWER_FULLY_LOADED_IND: VARCHAR2(3) NULL
COMMENTS: VARCHAR2(2000) NULL
LOCATION_ACCURACY: VARCHARZ2(25) NOT NULL (FK)
LOCATION_DESCR: VARCHAR2(2000) NULL
GEOG_UNIT_DESCR: VARCHAR2(2000) NULL
SENSITIVITY_CLASS: VARCHAR2(15) NOT NULL
SENSITIVITY_DATE: DATE NOT NULL
SENSITIVITY_RATIONALE: VARCHAR2(50) NOT NULL
SENS_RATIONALE_OTHER_DESCR: VARCHAR2(250) NULL
VERFICATION_STATUS_FLG: VARCHAR2(10) NULL
VERFICATION_STATUS_DATE: DATE NULL
BUSINESS_EFF_DATE_FLG: VARCHAR2(10)NULL
BUSINESS_EFFECTVE_DATE: DATE NULL.
BUSINESS_EXPIRY_DATE: DATE NULL
SYSTEM_CALCULATED_AREA: NUMBER(16:3) NULL
SYSTEM_CALCULATED_LENGTH: NUMBER(163) NULL
USER_CALCULATED_METRIC: NUMBER(16,3) NULL
GENERAL_COMMENTS: VARCHAR2(2000) NULL.
GEOMETRY_UPDATE_DATETIME: DATENULL
EFFECTIVE_DATETIME: DATE NOT NULL
SYSTEM_DATETIME: DATE NOT NULL

SHAPE: SDO_GEOMETRY NULL

LOCATION_ACCURACY_LIST
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